{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["仮設材注文表","マクロの解除について"],"not_rendered":{"charts":0,"images":6,"macros":1,"external_links":1,"defined_names":1,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"仮設材注文表","index":0,"n_rows":67,"n_cols":30,"rows_kept":67,"cut":false,"hidden":false,"merged":[[64,17,65,19],[62,1,65,1],[62,11,63,11],[63,6,65,6],[64,16,65,16],[54,16,55,16],[57,1,59,1],[57,6,59,6],[58,11,61,11],[58,16,59,16],[60,6,61,6],[60,16,61,16],[52,6,56,6],[52,11,53,11],[52,16,53,16],[54,11,57,11],[34,6,35,6],[31,11,32,11],[31,16,38,16],[47,11,48,11],[49,6,51,6],[33,11,34,11],[15,22,15,23],[17,6,18,6],[19,6,20,6],[20,16,21,16],[21,11,26,11],[25,16,26,16],[21,6,26,6],[13,6,16,6],[14,11,20,11],[15,16,17,16],[66,1,67,1],[66,2,66,19],[67,2,67,19],[33,1,35,1],[36,1,47,1],[27,6,33,6],[39,16,41,16],[42,6,43,6],[43,11,46,11],[44,6,46,6],[45,16,46,16],[36,6,37,6],[36,11,39,11],[38,6,41,6],[27,16,30,16],[28,11,30,11],[3,14,3,16],[4,14,4,16],[3,17,3,19],[3,4,3,6],[4,4,4,6],[3,7,3,9],[4,7,4,9],[4,17,4,19],[3,11,3,12],[4,1,4,2],[3,1,3,2],[5,1,7,1],[5,6,8,6],[23,1,32,1],[18,1,19,1],[20,1,21,1],[5,11,7,11],[5,16,14,16],[8,1,17,1],[8,11,13,11],[9,6,12,6],[0,16,0,19],[0,9,0,11],[1,1,1,4],[2,6,2,11],[2,1,2,4],[1,16,1,19],[2,16,2,19],[1,12,1,14],[1,6,1,11],[2,12,2,14]]}
[null,null,null,null,null,null,null,null,null,"仮設材注文表",null,null,null,null,"注文日",null,null,null,null,null,null,null,null,null,null,"★Excelで数量を入力する場合の注意点★"]
[null,"業者名",null,null,null,null,"現場名",null,null,null,null,null,"担当者",null,null,null,"連絡先",null,null,null,"電話番号"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"⇐ この全削除ボタンを押すと入力したセル全て"]
[null,"配車",null,null,"車種",null,null,"大型車進入",null,null,null,"進入可能車両",null,null,"納入日",null,null,"時間",null,null,null,null,null,null,null,"　　リセットされます。(空白になります)"]
[null,null,null,null,null,null,null,null,null,null,null,null,"まで"]
[null,"門型 ",1217,19.2,null,{"$f":"IF(E6=\"\",\"\",D6*E6)","v":""},"下桟　",1800,"2.1",null,{"$f":"IF(J6=\"\",\"\",I6*J6)","v":""},"作業用踏台",null,27.1,null,{"$f":"IF(O6=\"\",\"\",N6*O6)","v":""},"単管\nポール　","5.0",13.65,null,{"$f":"IF(T6=\"\",\"\",S6*T6)","v":""},null,-3.3,{"$f":"W6*T6","v":0},null,"黄色に色付けされた部分はプルダウンで選択してください。","自社手配","軽トラック","可能","軽トラック"]
[null,null,"0917",16.2,null,"",null,1500,"1.8",null,"",null,"階段手摺",1.8,null,"",null,4.5,12.29,null,"",null,-2.92,0,null,"配車を自社手配にされた場合、車種・大型車進入・進入可能車両の","組合手配","2ｔ平","不可","2ｔ平"]
[null,null,"0617",15,null,"",null,1200,"1.5",null,"",null,"天板手摺",2.7,null,"",null,"4.0",10.92,null,"",null,-2.6,0,null,"選択は不要です。",null,"3ｔ平",null,"3ｔ平"]
[null,"調整枠　　",1212,16.2,null,"",null,"900",1.1000000000000001,null,"","サポート　","9尺",15.5,null,"",null,3.5,9.5549999999999997,null,"",null,-2.2749999999999999,0,null,null,null,"3ｔユニック",null,"3ｔユニック"]
[null,null,1209,13.3,null,"","巾木",1800,"4.6",null,"",null,"7尺",13.7,null,"",null,"3.0",8.19,null,"",null,-1.95,0,null,"組合手配の場合、7tユニックを代車で手配する場合が多々あります。",null,"4ｔ平",null,"4ｔ平"]
[null,null,"1205",9.1999999999999993,null,"",null,1500,"4.1",null,"",null,"6尺",12.9,null,"",null,2.5,6.8250000000000002,null,"",null,-1.625,0,null,"車がスムーズに手配できるようにお手数ですが全ての項目の選択をお願いいたします。",null,"4ｔユニック",null,"4ｔユニック"]
[null,null,"0915",15.2,null,"",null,1200,"3.5",null,"",null,"4尺",8.5,null,"",null,"2.0",5.46,null,"",null,-1.3,0,null,"ただし、選択して頂いた車種を手配できるとは限りませんのでご了承ください。",null,"5ｔ平",null,"5ｔ平"]
[null,null,"0912",14.5,null,"",null,900,"3.0",null,"",null,"3尺",6.6,null,"",null,1.5,4.0999999999999996,null,"",null,-0.97499999999999998,0,null,null,null,"5ｔユニック",null,"5ｔユニック"]
[null,null,"0909",10.7,null,"","ﾗｲﾌｶﾞｰﾄﾞ　　　",1800,13,null,"",null,"2尺",5.6,null,"",null,"1.0",2.73,null,"",null,-0.65,0,null,"★納入日・注文日",null,"7ｔ平"]
[null,null,"0905",7.8,null,"",null,1500,12.1,null,"","60角バタ　　","4.0",16.239999999999998,null,"",null,0.5,1.365,null,"",null,-0.32500000000000001,0,null,"コメントを入力していますが、11月20日と入力したい場合は11/20と入力してください。",null,"7ｔ平ユニック"]
[null,null,"0612",11.7,null,"",null,1200,11.2,null,"",null,3.5,14.21,null,"","兼用\nクランプ　　　　　","直交","0.8",null,"",null,{"$f":"SUM(X6:X15)/1000","v":0},null,null,"翌年の日付に関しては2023/11/20のように西暦から入力をお願いします。",null,"8ｔユニック"]
[null,null,"0609",9.1999999999999993,null,"",null,900,10.3,null,"",null,"3.0",12.18,null,"",null,"自在",0.8,null,"",null,null,null,null,null,null,"10ｔ平"]
[null,null,"0605",7.2,null,"","鋼製脚立　　　　","6尺",18,null,"",null,2.5,10.15,null,"",null,"ｷｬｯﾁ",1.1200000000000001,null,"",null,null,null,null,"★時間",null,"10ｔユニック"]
["※","簡易枠","0617 A",13.5,null,"",null,"4尺",15,null,"",null,"2.0",8.1199999999999992,null,"","ジョイント",null,0.625,null,"",null,null,null,null,"コメントを入力していますが、10時30分着の場合は10：30と入力してください。",null,"15ｔ平"]
["※",null,"0617 B",13.5,null,"","アルミ脚立","6尺",11.6,null,"",null,1.5,6.09,null,"","ﾍﾞｰｽﾌﾟﾚｰﾄ",null,0.81499999999999995,null,"",null,null,null,null,"10時着の場合は10：00と入力。時、分着については自動で付きます。"]
[null,"ﾌﾞﾗｹｯﾄ枠","0912",19.7,null,"",null,"4尺",7.6,null,"",null,"1.0",4.0599999999999996,null,"","三連\nクランプ","直交",1,null,""]
[null,null,"0609",17.8,null,"","勇馬","18号",23.3,null,"","100角バタ","4.0",38.1,null,"",null,"自在",1,null,"",null,null,null,null,"※簡易枠について(AかBを選んで数量記入お願いします)"]
[null,"梯子枠","1217",20.5,null,"",null,"14号",21.4,null,"",null,"3.0",28.6,null,"","枠上ベース",null,"0.6",null,"",null,null,null,null,"当組合保有の簡易枠が数種類あり、それぞれピンの位置が違います。"]
[null,"板布　　　","0518",16,null,"",null,"11号",16.2,null,"",null,"2.5",23.8,null,"","ｼｰﾄｸﾗﾝﾌﾟ",null,0.4,null,"",null,null,null,null,"Aは他の門型枠・調整枠等とピンの高さが同じため他の枠と共用可能です"]
[null,null,"0218",8.3000000000000007,null,"",null,"手摺",1.3,null,"",null,"2.0",19.100000000000001,null,"","ﾈｯﾄｸﾗﾝﾌﾟ",null,0.83,null,"",null,null,null,null,"Bは他の枠とピンの高さが違うため単独でのみ使用可能です※他の枠と共用不可です"]
[null,null,"0515",13.5,null,"",null,"補助ｽﾃｰｼﾞ",0.53,null,"",null,"1.5",14.3,null,"","根がらみ\nクランプ","直交",0.8,null,""]
[null,null,"0215",6.9,null,"",null,"ブリッジ",8.5,null,"",null,"1.0",9.52,null,"",null,"自在",0.8,null,""]
[null,null,"0512",10.4,null,"","ラクラクダイ","Ｌ",65,null,"","100角ジョイント",null,2.93,null,"","養生ｸﾗﾝﾌﾟ","427",0.5,null,""]
[null,null,"0212",5.9,null,"",null,"М",60,null,"","ｸﾛｽｹﾞｰﾄ　　　","5m",120,null,"",null,486,0.5,null,""]
[null,null,"0509",8.4,null,"",null,"手摺大",7,null,"",null,"4m",100,null,"","養生兼用","兼用",0.5,null,""]
[null,null,"0209",5.0999999999999996,null,"",null,"手摺小",5,null,"",null,"3m",80,null,"",null,"コーナー",0.5,null,""]
[null,null,"0506",5.8,null,"",null,"L用梯子",5,null,"","万能板　　　　",5430,18.100000000000001,null,"","壁つなぎ　　　","A1000",2.2999999999999998,null,""]
[null,null,"0206",3.5,null,"",null,"M用梯子",4.5,null,"",null,"5420",12.1,null,"",null,"A800",1.72,null,""]
[null,"ハッチ式板布","1800",16,null,"",null,"ブリッジ",12,null,"","パンチング　　　",5430,14.2,null,"",null,"A600",1.45,null,""]
[null,null,"1500",15,null,"","ベランダ\nステップ　　　",null,14,null,"",null,5420,9.6999999999999993,null,"",null,"A400",1.1399999999999999,null,""]
[null,null,"1200",13,null,"",null,"  手摺",4,null,"","フックボルト",null,7.0000000000000007E-2,null,"",null,"A350",1.02,null,""]
[null,"ブレース　　　　",1812,4.0999999999999996,null,"","垂直ﾀﾗｯﾌﾟ\n(猿梯子)","427",7.5,null,"","チェーン　　　　　","5m",2.87,null,"",null,"A300",0.96,null,""]
[null,null,1512,3.6,null,"",null,"486",7.5,null,"",null,"4m","2.32",null,"",null,"A200",0.9,null,""]
[null,null,1212,3.1,null,"","養生枠　",1800,10,null,"",null,"3m","1.77",null,"",null,"A160",0.8,null,""]
[null,null,"0912",2.7,null,"",null,1500,7.7,null,"",null,"2m","1.22",null,"","ﾒｯｼｭｼｰﾄ　　　　　　　　　",1.8,5,null,""]
[null,null,"0612",2.6,null,"",null,1200,6.6,null,"","ﾁｪｰﾝｸﾗﾝﾌﾟ",null,"0.6",null,"",null,1.5,"4.1",null,""]
[null,null,1804,3.5,null,"",null,900,5.3,null,"","親綱支柱","ｱﾙﾐ",6.4,null,"",null,1.2,"3.3",null,""]
[null,null,1504,2.9,null,"","隙間板       ",500,6,null,"","ｽﾀﾝｼｮﾝ","NRE",7.1,null,"","有",0.9,"2.5",null,""]
[null,null,1204,2.2999999999999998,null,"",null,250,3,null,"","緊付親綱　　","15ｍ",4.3499999999999996,null,{"$f":"IF(O44=\"\",\"\",N44*O44)","v":""},"無",0.6,"1.7",null,""]
[null,null,"0904",1.8,null,"","ローリング　　　　","枠","10.5",null,"",null,"10ｍ",3.35,null,"",{"$f":"SUM(T40:T45)*25","v":0},"0.3",1,null,""]
[null,null,1803,3.5,null,"",null,"桟","0.7",null,"",null,"8ｍ",3.15,null,"","防音ｼｰﾄ","1.8",9.8000000000000007,null,""]
[null,null,"1503",2.9,null,"",null,"巾木","6.2",null,"",null,"6ｍ",2.8,null,"",null,"1.5",8.1999999999999993,null,""]
[null,null,"1203",2.2000000000000002,null,"","キャスター",null,3.8,null,"","鉄筋フック","1型","0.63",null,"","有","1.2",6.5,null,""]
[null,null,"0903",1.7,null,"","ｼﾞｬｯｷ付ｷｬｽﾀｰ",null,5.25,null,"",null,"2型","0.92",null,"","無","0.9",4.9000000000000004,null,"",null,null,null,null,"★メッシュシート・防音シート"]
[null,"ｼﾞｬｯｷ",null,4.2,null,"","ｱｳﾄﾘｶﾞｰ　　",null,"9.8",null,"","ｸｲｯｸﾌﾞﾗｹｯﾄ",null,3,null,"",{"$f":"SUM(T46:T50)*30","v":0},"0.6",3.3,null,"",null,null,null,null,"紐が必要な場合は有に〇、不要な場合は無に〇をお願いします。"]
[null,"ﾛﾝｸﾞｼﾞｬｯｷ",null,4.9000000000000004,null,"",null,"ｼﾞｬｯｷ","5.6",null,"","アングルブラケット","1400",63,null,"","採光防音","1.8","10",null,"",null,null,null,null,"有に〇をした場合、無の下に表示された数量を納品しますので、希望数量と相違あれば"]
[null,"自在ｼﾞｬｯｷ",null,3.8,null,"",null,"一体型",11.5,null,"","単管ﾊﾞﾘｹｰﾄﾞ",null,"5.4",null,"","ｴﾚﾍﾞｰﾀｰﾋﾞｰﾑ","S",14.5,null,"",null,null,null,null,"数量を100本単位で入力してください。"]
[null,"大引受ｼﾞｬｯｷ",null,5.5,null,"","ペコビーム　　","1009",25.6,null,"","足場板　　　　","4.0",11,null,"","打込Tﾎﾟｰﾙ","1.5",4.0949999999999998,null,""]
[null,"大引受ﾛﾝｸﾞ",null,6.5,null,"",null,1007,20.399999999999999,null,"",null,"2.0",5.5,null,"",null,"1.0",2.73,null,""]
[null,"階段アルミ",null,11,null,"",null,1005,16.7,null,"","鋼製\n足場板　　","4.0","14.6",null,"","くい丸","1.5",4,null,""]
[null,"ｽﾃｯﾌﾟｶﾞｰド",null,14.8,null,"",null,2009,28,null,"",null,"3.0","11.2",null,"",null,"1.1",3,null,"",null,null,null,null,"★注文表をFAXで送る場合★"]
[null,"ｺｰﾅｰｶﾞｰﾄﾞ",null,3.2,null,"",null,2005,14.4,null,"",null,"2.0","7.8",null,"","木製巾木","4.0",3.7,null,"",null,null,null,null,"FAXの際、色付き部分の字が見えにくくなるため、印刷は白黒印刷になるよう"]
[null,"ブラケット  　","71",6.8,null,"","梁枠(1本)　　　　","4ｽﾊﾟﾝ","28",null,"",null,"1.0",4.2,null,"","コッパ板",null,0.55000000000000004,null,"",null,null,null,null,"設定しております。"]
[null,null,"57",4.8,null,"",null,"3ｽﾊﾟﾝ","41",null,"","アルミ板","4.0",7.6,null,"","アルウォーク","角バタ用",5.4,null,"",null,null,null,null,"設定変更をしてカラーで印刷をしないようにしてください。"]
[null,null,"35",4.0999999999999996,null,"",null,"2ｽﾊﾟﾝ","28",null,"",null,"3.0",5.7,null,"",null,"フック無",4.3,null,""]
[null,"ﾌﾞﾗｹｯﾄｸﾗﾝﾌﾟなし","35",4,null,"","方杖　　　　　　","3ｽﾊﾟﾝ",7,null,"",null,"2.0",3.9,null,"","ﾒｯｼｭﾊﾟﾚｯﾄ",null,84,null,"",null,null,null,null,"ＰＤＦでメールに添付する場合はカラーでも結構です。"]
[null,"手摺柱",null,3.1,null,"",null,"2ｽﾊﾟﾝ",5.5,null,"",null,"1.0",1.9,null,"",null,"吊り用",103,null,"",null,null,null,null,"印刷プレビューのページ設定よりシートタブを選び、白黒印刷のチェックを外すと"]
[null,"手摺桟　",1800,1.8,null,"","隅受",null,3,null,"","敷板　　　　　　","4.0",11,null,"","単クランプ","ﾎﾞﾙﾄ有・無",0.3,null,"",null,null,null,null,"カラー印刷となります。"]
[null,null,1500,1.5,null,"","梁渡\nピン要　　　",1217,6,null,"",null,"2.0",5.5,null,"","OKマット",null,6.52,null,""]
[null,null,1200,1.2,null,"",null,"0917",5,null,"","足場ステップ","600",6.5,null,"","合　計",{"$f":"SUM(F6:F66,K6:K66,P6:P66,U6:U64)/1000","v":0},null,null,""]
[null,null,"900","0.9",null,"",null,"0617",4,null,"","足場ｽﾃｯﾌﾟ(ﾜｲﾄﾞ)","900",6.4,null,""]
[null,"備考"]

{"sheet":"マクロの解除について","index":1,"n_rows":24,"n_cols":1,"rows_kept":24,"cut":false,"hidden":false,"merged":[]}
["注文表を開くと下記のように保護ビューで開くと思います。"]
["編集を有効にするをクリックしてください。"]
[]
[]
[]
[]
[]
[]
[]
["編集をクリック後、読み取り専用で開かれマクロの実行がブロックされた状態になります。"]
["このまま使用することも可能ですが、全削除ボタンが使用できません。"]
["全削除ボタンを使用できるようにするために、マクロの解除が必要です。"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["★マクロの解除方法★"]
["ファイルを一度閉じて、保存した場所でファイルを右クリックし、プロパティをクリックしてください。"]
["全般タブの下部にあるセキュリティの許可するにチェック☑をし、OKボタンをクリックしてください。"]